,EAN##OTHER##, Nominal Wattage##ELECTRICAL_WATTAGE##WATTS, Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS, Color Temperature##COLOR_TEMPERATURE##KELVIN, Length##LENGTH##MILLIMETERS, Bracket Min##LENGTH##MILLIMETERS, Bracket Max##LENGTH##MILLIMETERS, Model##OTHER##, URL##OTHER##, GEO##OTHER##, IES Light Source##OTHER##
DP SLIM VALUE 1200 36 W 4000 K IP65 GY, 4058075066458, 36, 4000, 4000, 1200, 600, 1100, DAMP PROOF SLIM VALUE 1200 36 W 4000 K IP65 GY, https://www.ledvance.com/professional/search?query=4058075066458, DP_SLIM_VAL : 1200, IES_DATA_DP_SLIM_VAL : DP SLIM VALUE 1200 36 W 4000 K IP65 GY
DP SLIM VALUE 1200 36 W 6500 K IP65 GY, 4058075066472, 36, 4000, 6500, 1200, 600, 1100, DAMP PROOF SLIM VALUE 1200 36 W 6500 K IP65 GY, https://www.ledvance.com/professional/search?query=4058075066472, DP_SLIM_VAL : 1200, IES_DATA_DP_SLIM_VAL : DP SLIM VALUE 1200 36 W 6500 K IP65 GY
DP SLIM VALUE 1500 50 W 4000 K IP65 GY, 4058075066496, 50, 5500, 4000, 1500, 800, 1400, DAMP PROOF SLIM VALUE 1500 50 W 4000 K IP65 GY, https://www.ledvance.com/professional/search?query=4058075066496, DP_SLIM_VAL : 1500, IES_DATA_DP_SLIM_VAL : DP SLIM VALUE 1500 50 W 4000 K IP65 GY
DP SLIM VALUE 1500 50 W 6500 K IP65 GY, 4058075066519, 50, 5500, 6500, 1500, 800, 1400, DAMP PROOF SLIM VALUE 1500 50 W 6500 K IP65 GY, https://www.ledvance.com/professional/search?query=4058075066519, DP_SLIM_VAL : 1500, IES_DATA_DP_SLIM_VAL : DP SLIM VALUE 1500 50 W 6500 K IP65 GY
